Concure AV

**Aliphatic alcohol evaporative retarder for plastic concrete to reduce shrinkage cracks**

**1.00 Evaporative Retarder Compound**

**1.10 Concrete Surface**

1.11 The evaporative retarder compound should be applied to freshly laid concrete or render surfaces as a fine mist to completely cover the concrete surface. Each application is important and should be carried out after initial screeding. After the surface has been sprayed, proceed with normal floating. When working in extremely hot or dry conditions further applications of evaporative retarder should be made after each subsequent operation, such as wood floating and steel trowelling.

**1.20 Evaporative Retarder**

1.21 All designated areas are to have an aliphatic alcohol evaporative retarder compound applied at an even coverage rate of 10 m2/litre after diluting to the manufacturers recommendation.

**1.30** **Fosroc Concure AV** meets the product criteria and is approved.