Expoband® F

**Highly flexible, chemically resistant, joint bandage membrane system**

* 1. **Joint Bandage Membrane System**
  2. Where indicated on the drawings, joints shall be sealed / over-strapped with a flexible Polyolefine bandage membrane having a tensile strength greater than 10 N/mm2 and an elongation greater than 600% and comply with AS4020:2018
  3. The bandage membrane will be bonded to the substrate using the recommended two part epoxy paste adhesive according to the manufacturers product data sheet.
  4. **Fosroc Expoband F** and **Nitomortar AP** adhesive meets the performance criteria and approved for this application.